Compact tubular heat exchanger, in some cases less than half the size of a traditional plain tube HE.

Long running times due to turbulent flow substantially reducing fouling

Uniform thermal processing. (Spiral in the core and eddy’s at the periphery)

Higher working temperatures and pressures.

High response to cleaning‐in‐place.

Higher coefficients result in closer temperature approaches between product and service fluids.